
@Tdefault
실행기|version;0.74_SVN|0.73|0.72|0.71|0.70|0.65|0.72_CVS|0.74|Win31KOR|Win31ENG|Win98|0.74_SVN_new|Windows|ANEX86|SNES9X|FUSION|NP21|M88|0.74_3DFX;<INDEX>
DirectX 드라이버 사용|DirectX;true|false;<INDEX>
도스박스 메뉴 보이기|Menu;false|true;<INDEX>
상태저장 경로(SVN 전용)|SavePath;save;<SAVEPATH>

@Tsdl
전체화면으로 실행|fullscreen;true|false;<INDEX>
전체화면 더블버퍼링|fulldouble;false|true;<INDEX>
전체화면모드 해상도|fullresolution;original|desktop|640x480|800x600|1024x768|1280x960|1280x1024|1440x1080|852x480|1366x768|1680x1050|1920x1080|1920x1200;<INDEX>
윈도 모드 해상도|windowresolution;original|640x480|800x600|1024x768|1280x960|1280x1024|1440x1080|852x480|1366x768|1680x1050|1920x1080||1920x1200;<INDEX>
화면 출력 방식|output;surface|overlay|ddraw|openglnb|opengl|direct3d|openglhq;<INDEX>
클릭시 마우스 잠그기|autolock;true|false;<INDEX>
마우스 민감도|sensitivity;50|100|150|200|250|300|400|500|600|700|800|900|1000;<INDEX>
도스박스 콘솔창 보이기|waitonerror;true|false;<INDEX>
도스박스 우선순위|priority;highest|higher|normal|lower|lowest|highest`pause|higher`pause|normal`pause|lower`pause|lowest`pause;<INDEX>
도스박스 매퍼파일|mapperfile;mapper_1.txt|mapper_2.txt|mapper_3.txt|mapper_4.txt|mapper_5.txt|mapper_6.txt|mapper_simulation.txt|mapper_user.txt;<MAPPER>
사용자 심볼키 사용|usescancodes;true|false;<INDEX>
오버스캔 테두리|overscan;0|1|2|3|4|5|6|7|8|9|10;<INDEX>
픽셀 셰이더 종류|pixelshader;none|2xSaI.fx|2xSaI_sRGB.fx|2xSaL.fx|2xSaL2xAA.fx|2xSaLAA.fx|2xSaL_Ls.fx|4xSaL.fx|4xSoft.fx|4xSoft_PS3.0.fx|5xBR-v3.5b.fx|5xBR-v3.8a.fx|5xBR-v3.8b.fx|5xBR-v3.8c.fx|AdvancedAA.fx|bilinear.fx|Cartoon.fx|ColorSketch.fx|CRT-geom-blend.fx|CRT-geom-curved.fx|CRT-simple.D3D.br.fx|CRT-simple.D3D.fx|CRT.D3D.br.fx|CRT.D3D.fx|DotnBloom.D3D.fx|EGAfilter.fx|GS2x.fx|GS2xFilter.fx|Gs2xLS.fx|Gs2xSmartFilter.fx|GS2xSuper.fx|GS2xTwo.fx|GS4x.fx|GS4xColorScale.fx|GS4xFilter.fx|GS4xHqFilter.fx|GS4xScale.fx|GS4xSoft.fx|HQ2x.fx|Lanczos.fx|Lanczos12.fx|Lanczos16.fx|Matrix.fx|MCAmber.fx|MCGreen.fx|MCHerc.fx|MCOrange.fx|none.fx|point.fx|scale2x.fx|Scale2xPlus.fx|scale2x_ps14.fx|Scale4x.fx|SimpleAA.fx|Sketch.fx|Super2xSaI.fx|SuperEagle.fx|Tv.fx|;<INDEX>

@Tlog
로그 기록(SVN 전용)|log;false|true;<INDEX>
logfile|logfile;logfile.txt;<LOGFILE>
log vga|vga;true|false;<INDEX>
log vgagfx|vgagfx;true|false;<INDEX>
log vgamisc|vgamisc;true|false;<INDEX>
log int10|int10;true|false;<INDEX>
log sblaster|sblaster;true|false;<INDEX>
log dma_control|dma_control;true|false;<INDEX>
log fpu|fpu;true|false;<INDEX>
log cpu|cpu;true|false;<INDEX>
log paging|paging;true|false;<INDEX>
log fcb|fcb;true|false;<INDEX>
log files|files;true|false;<INDEX>
log ioctl|ioctl;true|false;<INDEX>
log exec|exec;true|false;<INDEX>
log dosmisc|dosmisc;true|false;<INDEX>
log keyboard|keyboard;true|false;<INDEX>
log pic|pic;true|false;<INDEX>
log mouse|mouse;true|false;<INDEX>
log bios|bios;true|false;<INDEX>
log gui|gui;true|false;<INDEX>
log misc|misc;true|false;<INDEX>
log io|io;true|false;<INDEX>
log pci|pci;true|false;<INDEX>
log sst|sst;true|false;<INDEX>

@Tdosbox
도스박스 언어파일|language; ;<NONE>
가상구현 기기|machine;hercules|cga|tandy|pcjr|ega|vgaonly|svga_s3|svga_et3000|svga_et4000|svga_paradise|vesa_nolfb|vesa_oldvbe|cga_mono|amstrad;<INDEX>
캡쳐(ctrl+F5) 위치|captures;dosbox;<CAPTURE>
메모리 용량|memsize;2|4|8|16|32|64|128|256|512;<INDEX>
VMEM 용량|vmemsize;4|0|1|2|8|16;<INDEX>
VMEM 추가 용량(kb)|vmemsizekb;0;<INDEX>
mainline compatible mapping|mainline compatible mapping;true|false;<INDEX>
mainline compatible bios mapping|mainline compatible bios mapping;true|false;<INDEX>
adapter rom is ram|adapter rom is ram;false|true;<INDEX>
shell environment size|shell environment size;0;<INDEX>
private area size|private area size;32768;<INDEX>
a20|a20;fast|mask|off|on|off_fake|on_fake;<INDEX>
isa bus clock|isa bus clock;std8.3|std8|std6|std4.77|oc10|oc12|oc15|oc16;<INDEX>
pci bus clock|pci bus clock;std33.3|std30|std25;<INDEX>
rom bios allocation max|rom bios allocation max;0;<INDEX>
rom bios minimum size|rom bios minimum size;0;<INDEX>
메모리 추가 용량(kb)|memsizekb;0;<INDEX>
memalias|memalias;0|24|26;<INDEX>
vga bios size override|vga bios size override;0;<INDEX>
video bios dont duplicate cga first half rom font|video bios dont duplicate cga first half rom font;false|true;<INDEX>
video bios always offer 14-pixel high rom font|video bios always offer 14-pixel high rom font;true|false;<INDEX>
video bios always offer 16-pixel high rom font|video bios always offer 16-pixel high rom font;true|false;<INDEX>
video bios enable cga second half rom font|video bios enable cga second half rom font;true|false;<INDEX>
forcerate|forcerate;0|50|60;<INDEX>
sierra ramdac|sierra ramdac;true|false;<INDEX>
sierra ramdac lock 565|sierra ramdac lock 565;false|true;<INDEX>
page flip debug line|page flip debug line;false|true;<INDEX>
vertical retrace poll debug line|vertical retrace poll debug line;false|true;<INDEX>
CGA 스노우 모드|cgasnow;true|false;<INDEX>
allow port 92 reset|allow port 92 reset;true|false;<INDEX>
enable port 92|enable port 92;true|false;<INDEX>
enable 1st dma controller|enable 1st dma controller;true|false;<INDEX>
enable 2nd dma controller|enable 2nd dma controller;true|false;<INDEX>
allow dma address decrement|allow dma address decrement;true|false;<INDEX>
enable dma extra page registers|enable dma extra page registers;true|false;<INDEX>
dma page registers write-only|dma page registers write-only;false|true;<INDEX>
enable slave pic|enable slave pic;true|false;<INDEX>
enable pc nmi mask|enable pc nmi mask;true|false;<INDEX>
rom bios 8x8 CGA font|rom bios 8x8 CGA font;true|false;<INDEX>
rom bios video parameter table|rom bios video parameter table;true|false;<INDEX>
allow more than 640kb base memory|allow more than 640kb base memory;false|true;<INDEX>
vesa lfb base scanline adjust|vesa lfb base scanline adjust;0|1|2|3|4|5|6|&|8|9|10;<INDEX>
allow hpel effects|allow hpel effects;false|true;<INDEX>
allow hretrace effects|allow hretrace effects;false|true;<INDEX>
hretrace effect weight|hretrace effect weight;4.00|6.00|8.00|10.00|12.00;<INDEX>
vesa vbe 1.2 modes are 32bpp|vesa vbe 1.2 modes are 32bpp;true|false;<INDEX>
allow 32bpp vesa modes|allow 32bpp vesa modes;true|false;<INDEX>
allow 24bpp vesa modes|allow 24bpp vesa modes;true|false;<INDEX>
allow 16bpp vesa modes|allow 16bpp vesa modes;true|false;<INDEX>
allow 15bpp vesa modes|allow 15bpp vesa modes;true|false;<INDEX>
allow 8bpp vesa modes|allow 8bpp vesa modes;true|false;<INDEX>
allow 4bpp vesa modes|allow 4bpp vesa modes;true|false;<INDEX>
allow tty vesa modes|allow tty vesa modes;true|false;<INDEX>
enable vga resize delay|enable vga resize delay;false|true;<INDEX>
enable pci bus|enable pci bus;true|false;<INDEX>
pit hack|pit hack;pc_speaker_as_timer|project_angel_demo;<INDEX>

@Trender
프레임 스킵|frameskip;0|1|2|3|4|5|6|7|8|9|10;<INDEX>
화면비를 고정|aspect;false|true;<INDEX>
출력 스케일러|scaler;none|hardware2x|hardware3x|advmame2x|advmame3x|advinterp2x|advinterp3x|hq2x|hq3x|2xsai|super2xsai|supereagle|tv2x|tv3x|rgb2x|rgb3x|scan2x|scan3x|normal2x|normal3x|xbrz|hardware2x forced|hardware3x forced|advmame2x forced|advmame3x forced|advinterp2x forced|advinterp3x forced|hq2x forced|hq3x forced|2xsai forced|super2xsai forced|supereagle forced|tv2x forced|tv3x forced|rgb2x forced|rgb3x forced|scan2x forced|scan3x forced|normal2x forced|normal3x forced|xbrz forced;<INDEX>
linewise|linewise;false|true;<INDEX>
char9|char9;false|true;<INDEX>
multiscan|multiscan;false|true;<INDEX>
doublescan|doublescan;false|true;<INDEX>
autofit|autofit;direct3d|original|true;<INDEX>

@Tvsync
수직동기화|vsyncmode;off|on|force|host;<INDEX>
수직동기화 재생 빈도|vsyncrate;60|65|70|75|80;<INDEX>

@Tcpu
CPU 코어|core;auto|dynamic|normal|full|simple|prefetch;<INDEX>
CPU 종류|cputype;auto|386|386_slow|486_slow|pentium_slow|386_prefetch|pentium|386|486|pentium_mmx;<INDEX>
CPU 속도|cycles;auto|max;<CPUCYCLE>
CPU 속도 증가폭(ctrl+F12)|cycleup;50|100|150|200|250|300|350|400|450|500;<INDEX>
CPU 속도 감소폭(ctrl+F11)|cycledown;50|100|150|200|250|300|350|400|450|500;<INDEX>
ISA PNP 바이오스|isapnpbios;true|false;<INDEX>
enable msr|enable msr;true|false;<INDEX>
ignore undefined msr|ignore undefined msr;false|true;<INDEX>
dynamic core cache block size|dynamic core cache block size;32|16|64;<INDEX>
non-recursive page fault|non-recursive page fault;false|true;<INDEX>
ignore opcode 63|ignore opcode 63;true|false;<INDEX>
apmbios|apmbios;false|true;<INDEX>
apmbios allow realmode|apmbios allow realmode;true|false;<INDEX>
apmbios allow 16-bit protected mode|apmbios allow 16-bit protected mode;true|false;<INDEX>
apmbios allow 32-bit protected mode|apmbios allow 32-bit protected mode;true|false;<INDEX>
integration device|integration device;false|true;<INDEX>
realbig16|realbig16;false|true;<INDEX>

@Tkeyboard
aux_|aux;false|true;<INDEX>
auxdevice|auxdevice;intellimouse|none|2button|3button|intellimouse45;<INDEX>
allow output port reset|allow output port reset;true|false;<INDEX>

@Tpci
PCI 부두장치|voodoo;auto|false|software|opengl;<INDEX>
부두장치 메모리|voodoomem;standard|max;<INDEX>

@Tmixer
음소거|nosound;true|false;<INDEX>
음질|rate;8000|11025|16000|22050|32000|44100|48000|49716;<INDEX>
블록크기|blocksize;256|512|1024|2048|4096|8192;<INDEX>
프리버퍼(밀리세컨드)|prebuffer;20|30|40|50;<INDEX>
믹서 좌우 바꾸기|swapstereo;false|true;<INDEX>
MASTER 볼륨|MASTER;100|10|20|30|40|50|60|70|80|90|150|200|250|300;<INDEX>
PC스피커 볼륨|SPKR;100|10|20|30|40|50|60|70|80|90|150|200|250|300;<INDEX>
GUS 볼륨|GUS;100|10|20|30|40|50|60|70|80|90|150|200|250|300;<INDEX>
SB 볼륨|SB;60|10|20|30|40|50|70|80|90|100|150|200|250|300;<INDEX>
FM 볼륨|FM;60|10|20|30|40|50|70|80|90|100|150|200|250|300;<INDEX>
MT32 볼륨|MT32;100|10|20|30|40|50|60|70|80|90|150|200|250|300;<INDEX>

@Tmidi
mpu401|mpu401;intelligent|uart|none;<INDEX>
미디 디바이스|mididevice;default|win32|alsa|oss|coreaudio|coremidi|mt32|synth|timidity|none;<INDEX>
미디 설정|midiconfig;0|1|2|3|4|5|6|7|8|9;<INDEX>
미디 좌우 바꾸기|mt32.reverse.stereo;off|on;<INDEX>
mt32 verbose|mt32.verbose;off|on;<INDEX>
mt32 Threading|mt32.thread;off|on;<INDEX>
MT32 DAC input mode|mt32.dac;auto|0|1|2|3;<INDEX>
mt32 reverb mode|mt32reverb.mode;auto|0|1|2|3;<INDEX>
mt32 reverb time|mt32reverb.time;5|0|1|2|3|4|6|7;<INDEX>
mt32 reverb level|mt32reverb.level;3|0|1|2|4|5|6|7;<INDEX>
mt32 Max Partials|mt32.partials;32|64|96|128|160|192|224|256;<INDEX>

@Tsblaster
SB 종류|sbtype;sb1|sb2|sbpro1|sbpro2|sb16|sb16vibra|gb|none;<INDEX>
SB base|sbbase;220|240|260|280|2a0|2c0|2e0|300;<INDEX>
SB irq|irq;3|5|7|9|10|11|12;<INDEX>
SB dma|dma;0|1|3|5|6|7;<INDEX>
SB hdma|hdma;0|1|3|5|6|7;<INDEX>
SB mixer|sbmixer;true|false;<INDEX>
SB oplmode|oplmode;auto|cms|opl2|dualopl2|opl3|none|hardware|hardwaregb;<INDEX>
SB oplemu|oplemu;default|compat|fast|old;<INDEX>
SB 음질|oplrate;8000|11025|16000|22050|32000|44100|48000|49716;<INDEX>
SB 하드웨어 base|hardwarebase;220|240|260|280|2a0|2c0|2e0|300;<INDEX>
SB goldplay 지원|goldplay;false|true;<INDEX>
force dsp auto-init|force dsp auto-init;false|true;<INDEX>
force goldplay|+force goldplay;false|true;<INDEX>
goldplay stereo|goldplay stereo;true|false;<INDEX>
dsp require interrupt acknowledge|dsp require interrupt acknowledge;auto|false;<INDEX>
dsp write busy delay|dsp write busy delay;-1;<INDEX>
blaster environment variable|blaster environment variable;true|false;<INDEX>
sample rate limits|sample rate limits;true|false;<INDEX>
instant direct dac|instant direct dac;false|true;<INDEX>
stereo control with sbpro only|stereo control with sbpro only;true|false;<INDEX>
dsp busy cycle rate|dsp busy cycle rate;-1;<INDEX>
dsp busy cycle duty|dsp busy cycle duty;-1;<INDEX>
io port aliasing|io port aliasing;true|false;<INDEX>

@Tgus
GUS 가상구현|gus;true|false;<INDEX>
GUS 음질|gusrate;8000|11025|16000|22050|32000|44100|48000|49716;<INDEX>
GUS base|gusbase;220|240|260|280|2a0|2c0|2e0|300;<INDEX>
GUS irq|gusirq;3|5|7|9|10|11|12;<INDEX>
GUS dma|gusdma;0|1|3|5|6|7;<INDEX>
GUS ultradir|ultradir;Y:\ULTRASND;<NONE>

@Tinnova
Innovation SSI-2001 가상구현|innova;false|true;<INDEX>
innova sample rate|samplerate;8000|11025|16000|22050|32000|44100|48000|49716;<INDEX>
innova sidbase|sidbase;220|240|260|280|2a0|2c0|2e0|300;<INDEX>
innova quality|quality;0|1|2|3;<INDEX>

@Tspeaker
PC스피커 가상구현 사용|pcspeaker;true|false;<INDEX>
PC스피커 음질|pcrate;8000|11025|16000|22050|32000|44100|48000|49716;<INDEX>
tandy 3-voice 사용|tandy;off|on|auto;<INDEX>
tandy 음질|tandyrate;8000|11025|16000|22050|32000|44100|48000|49716;<INDEX>
disney 사운드 소스 사용|disney;false|true;<INDEX>
IBM PS1 오디오 에뮬레이션|ps1audio;off|on|auto;<INDEX>
IBM PS1 오디오 음질|ps1audiorate;8000|11025|16000|22050|32000|44100|48000|49716;<INDEX>

@Tjoystick
조이스틱 타입|joysticktype;auto|none|2axis|4axis|4axis_2|fcs|ch;<INDEX>
timed|timed;true|false;<INDEX>
autofire|autofire;true|false;<INDEX>
swap34|swap34;true|false;<INDEX>
buttonwrap|buttonwrap;true|false;<INDEX>

@Tserial
serial1|serial1;dummy|disabled|modem|nullmodem|serialmouse|directserial;<INDEX>
serial2|serial2;dummy|disabled|modem|nullmodem|serialmouse|directserial;<INDEX>
serial3|serial3;dummy|disabled|modem|nullmodem|serialmouse|directserial;<INDEX>
serial4|serial4;dummy|disabled|modem|nullmodem|serialmouse|directserial;<INDEX>

@Tprinter
printer 에뮬레이션|printer;false|true;<INDEX>
dpi|dpi;360;<INDEX>
가로폭|width;85;<INDEX>
세로폭|height;110;<INDEX>
프린터 출력 형태|printoutput;png|bmp|ps|printer;<INDEX>
multipage|multipage;false|true;<INDEX>
출력파일 저장경로|docpath;dosbox;<DOCPATH>
timeout|timeout;0;<INDEX>

@Tparallel
parallel1|parallel1;disabled|reallpt|file|printer;<INDEX>
parallel2|parallel2;disabled|reallpt|file|printer;<INDEX>
parallel3|parallel3;disabled|reallpt|file|printer;<INDEX>
dongle|dongle;false|true;<INDEX>

@Tglide
글라이드 사용|glide;true|false|emu;<INDEX>
글라이드 IO 포트|grport;600;<INDEX>
글라이드 LFB 접근방식|lfb;full|full_noaux|read|read_noaux|write|write_noaux|none;<INDEX>
3DFX 스플래쉬 보기|splash;false|true;<INDEX>

@Tdos
xms 메모리 사용|xms;true|false;<INDEX>
ems 메모리 사용|ems;true|false;<INDEX>
umb 메모리 사용|umb;true|false;<INDEX>
키보드 레이아웃|keyboardlayout;auto|none;<INDEX>
ems system handle memory size|ems system handle memory size;384;<INDEX>
umb start|umb start;0;<INDEX>
umb end|umb end;0;<INDEX>
kernel allocation in umb|kernel allocation in umb;false|true;<INDEX>
dynamic kernel allocation|dynamic kernel allocation;false|true;<INDEX>
keep umb on boot|keep umb on boot;false|true;<INDEX>
keep private area on boot|keep private area on boot;false|true;<INDEX>
private area in umb|private area in umb;true|false;<INDEX>
automount|automount;true|false;<INDEX>
int33|int33;true|false;<INDEX>
int 13 extensions|int 13 extensions;true|false;<INDEX>
biosps2|biosps2;true|false;<INDEX>
int15 mouse callback does not preserve registers|int15 mouse callback does not preserve registers;false|true;<INDEX>
dbcs|dbcs;true|false;<INDEX>
filenamechar|filenamechar;true|false;<INDEX>
collating and uppercase|collating and uppercase;true|false;<INDEX>
files|files;127;<INDEX>

@Tne2000
ne2000|ne2000;false|true;<INDEX>
nicbase|nicbase;300;<INDEX>
nicirq|nicirq;3;<INDEX>
macaddr|macaddr;AC:DE:48:88:99:AA;<INDEX>
realnic|realnic;list|1|2|3|4|5;<INDEX>

@Tfdc` primary
fdc enable|enable;false|true;<INDEX>
fdc pnp|pnp;true|false;<INDEX>
fdc irq|irq;0|1|2|3|4|5|6;<INDEX>
fdc io|io;0|1|2|3|4|5|6;<INDEX>
fdc dma|dma;-1|0|1|2|3|4|5|6;<INDEX>
fdc int13fakev86io|int13fakev86io;false|true;<INDEX>
fdc instant mode|instant mode;false|true;<INDEX>
fdc auto-attach to int 13h|auto-attach to int 13h;true|false;<INDEX>
fdc mode|mode;ps2|ps2_model30|at|xt;<INDEX>
fdc chip|chip;82077aa|82072|nec_uPD765|none;<INDEX>

@Tfdc` secondary
fdc enable|enable;false|true;<INDEX>
fdc pnp|pnp;true|false;<INDEX>
fdc irq|irq;0|1|2|3|4|5|6;<INDEX>
fdc io|io;0|1|2|3|4|5|6;<INDEX>
fdc dma|dma;-1|0|1|2|3|4|5|6;<INDEX>
fdc int13fakev86io|int13fakev86io;false|true;<INDEX>
fdc instant mode|instant mode;false|true;<INDEX>
fdc auto-attach to int 13h|auto-attach to int 13h;true|false;<INDEX>
fdc mode|mode;ps2|ps2_model30|at|xt;<INDEX>
fdc chip|chip;82077aa|82072|nec_uPD765|none;<INDEX>

@Tfdc` tertiary
fdc enable|enable;false|true;<INDEX>
fdc pnp|pnp;true|false;<INDEX>
fdc irq|irq;0|1|2|3|4|5|6;<INDEX>
fdc io|io;0|1|2|3|4|5|6;<INDEX>
fdc dma|dma;-1|0|1|2|3|4|5|6;<INDEX>
fdc int13fakev86io|int13fakev86io;false|true;<INDEX>
fdc instant mode|instant mode;false|true;<INDEX>
fdc auto-attach to int 13h|auto-attach to int 13h;true|false;<INDEX>
fdc mode|mode;ps2|ps2_model30|at|xt;<INDEX>
fdc chip|chip;82077aa|82072|nec_uPD765|none;<INDEX>

@Tfdc` quaternary
fdc enable|enable;false|true;<INDEX>
fdc pnp|pnp;true|false;<INDEX>
fdc irq|irq;0|1|2|3|4|5|6;<INDEX>
fdc io|io;0|1|2|3|4|5|6;<INDEX>
fdc dma|dma;-1|0|1|2|3|4|5|6;<INDEX>
fdc int13fakev86io|int13fakev86io;false|true;<INDEX>
fdc instant mode|instant mode;false|true;<INDEX>
fdc auto-attach to int 13h|auto-attach to int 13h;true|false;<INDEX>
fdc mode|mode;ps2|ps2_model30|at|xt;<INDEX>
fdc chip|chip;82077aa|82072|nec_uPD765|none;<INDEX>

@Tfdc` quinternary
fdc enable|enable;false|true;<INDEX>
fdc pnp|pnp;true|false;<INDEX>
fdc irq|irq;0|1|2|3|4|5|6;<INDEX>
fdc io|io;0|1|2|3|4|5|6;<INDEX>
fdc dma|dma;-1|0|1|2|3|4|5|6;<INDEX>
fdc int13fakev86io|int13fakev86io;false|true;<INDEX>
fdc instant mode|instant mode;false|true;<INDEX>
fdc auto-attach to int 13h|auto-attach to int 13h;true|false;<INDEX>
fdc mode|mode;ps2|ps2_model30|at|xt;<INDEX>
fdc chip|chip;82077aa|82072|nec_uPD765|none;<INDEX>

@Tfdc` sexternary
fdc enable|enable;false|true;<INDEX>
fdc pnp|pnp;true|false;<INDEX>
fdc irq|irq;0|1|2|3|4|5|6;<INDEX>
fdc io|io;0|1|2|3|4|5|6;<INDEX>
fdc dma|dma;-1|0|1|2|3|4|5|6;<INDEX>
fdc int13fakev86io|int13fakev86io;false|true;<INDEX>
fdc instant mode|instant mode;false|true;<INDEX>
fdc auto-attach to int 13h|auto-attach to int 13h;true|false;<INDEX>
fdc mode|mode;ps2|ps2_model30|at|xt;<INDEX>
fdc chip|chip;82077aa|82072|nec_uPD765|none;<INDEX>

@Tfdc` septernary
fdc enable|enable;false|true;<INDEX>
fdc pnp|pnp;true|false;<INDEX>
fdc irq|irq;0|1|2|3|4|5|6;<INDEX>
fdc io|io;0|1|2|3|4|5|6;<INDEX>
fdc dma|dma;-1|0|1|2|3|4|5|6;<INDEX>
fdc int13fakev86io|int13fakev86io;false|true;<INDEX>
fdc instant mode|instant mode;false|true;<INDEX>
fdc auto-attach to int 13h|auto-attach to int 13h;true|false;<INDEX>
fdc mode|mode;ps2|ps2_model30|at|xt;<INDEX>
fdc chip|chip;82077aa|82072|nec_uPD765|none;<INDEX>

@Tfdc` octernary
fdc enable|enable;false|true;<INDEX>
fdc pnp|pnp;true|false;<INDEX>
fdc irq|irq;0|1|2|3|4|5|6;<INDEX>
fdc io|io;0|1|2|3|4|5|6;<INDEX>
fdc dma|dma;-1|0|1|2|3|4|5|6;<INDEX>
fdc int13fakev86io|int13fakev86io;false|true;<INDEX>
fdc instant mode|instant mode;false|true;<INDEX>
fdc auto-attach to int 13h|auto-attach to int 13h;true|false;<INDEX>
fdc mode|mode;ps2|ps2_model30|at|xt;<INDEX>
fdc chip|chip;82077aa|82072|nec_uPD765|none;<INDEX>

@Tide` primary
ide enable|enable;true|false;<INDEX>
ide pnp|pnp;true|false;<INDEX>
ide irq|irq;0|1|2|3|4|5|6;<INDEX>
ide io|io;0|1F0;<INDEX>
ide altio|altio;0|3F6;<INDEX>
ide int13fakeio|int13fakeio;false|true;<INDEX>
ide int13fakev86io|int13fakev86io;false|true;<INDEX>
ide enable pio32|enable pio32;false|true;<INDEX>
ide ignore pio32|ignore pio32;false|true;<INDEX>
ide cd-rom spinup time|cd-rom spinup time;0;<INDEX>
ide cd-rom spindown timeout|cd-rom spindown timeout;0;<INDEX>
ide cd-rom insertion delay|cd-rom insertion delay;0;<INDEX>

@Tide` secondary
ide enable|enable;true|false;<INDEX>
ide pnp|pnp;true|false;<INDEX>
ide irq|irq;0|1|2|3|4|5|6;<INDEX>
ide io|io;0|1F0;<INDEX>
ide altio|altio;0|3F6;<INDEX>
ide int13fakeio|int13fakeio;false|true;<INDEX>
ide int13fakev86io|int13fakev86io;false|true;<INDEX>
ide enable pio32|enable pio32;false|true;<INDEX>
ide ignore pio32|ignore pio32;false|true;<INDEX>
ide cd-rom spinup time|cd-rom spinup time;0;<INDEX>
ide cd-rom spindown timeout|cd-rom spindown timeout;0;<INDEX>
ide cd-rom insertion delay|cd-rom insertion delay;0;<INDEX>

@Tide` tertiary
ide enable|enable;false|true;<INDEX>
ide pnp|pnp;true|false;<INDEX>
ide irq|irq;0|1|2|3|4|5|6;<INDEX>
ide io|io;0|1F0;<INDEX>
ide altio|altio;0|3F6;<INDEX>
ide int13fakeio|int13fakeio;false|true;<INDEX>
ide int13fakev86io|int13fakev86io;false|true;<INDEX>
ide enable pio32|enable pio32;false|true;<INDEX>
ide ignore pio32|ignore pio32;false|true;<INDEX>
ide cd-rom spinup time|cd-rom spinup time;0;<INDEX>
ide cd-rom spindown timeout|cd-rom spindown timeout;0;<INDEX>
ide cd-rom insertion delay|cd-rom insertion delay;0;<INDEX>

@Tide` quaternary
ide enable|enable;false|true;<INDEX>
ide pnp|pnp;true|false;<INDEX>
ide irq|irq;0|1|2|3|4|5|6;<INDEX>
ide io|io;0|1F0;<INDEX>
ide altio|altio;0|3F6;<INDEX>
ide int13fakeio|int13fakeio;false|true;<INDEX>
ide int13fakev86io|int13fakev86io;false|true;<INDEX>
ide enable pio32|enable pio32;false|true;<INDEX>
ide ignore pio32|ignore pio32;false|true;<INDEX>
ide cd-rom spinup time|cd-rom spinup time;0;<INDEX>
ide cd-rom spindown timeout|cd-rom spindown timeout;0;<INDEX>
ide cd-rom insertion delay|cd-rom insertion delay;0;<INDEX>

@Tide` quinternary
ide enable|enable;false|true;<INDEX>
ide pnp|pnp;true|false;<INDEX>
ide irq|irq;0|1|2|3|4|5|6;<INDEX>
ide io|io;0|1F0;<INDEX>
ide altio|altio;0|3F6;<INDEX>
ide int13fakeio|int13fakeio;false|true;<INDEX>
ide int13fakev86io|int13fakev86io;false|true;<INDEX>
ide enable pio32|enable pio32;false|true;<INDEX>
ide ignore pio32|ignore pio32;false|true;<INDEX>
ide cd-rom spinup time|cd-rom spinup time;0;<INDEX>
ide cd-rom spindown timeout|cd-rom spindown timeout;0;<INDEX>
ide cd-rom insertion delay|cd-rom insertion delay;0;<INDEX>

@Tide` sexternary
ide enable|enable;false|true;<INDEX>
ide pnp|pnp;true|false;<INDEX>
ide irq|irq;0|1|2|3|4|5|6;<INDEX>
ide io|io;0|1F0;<INDEX>
ide altio|altio;0|3F6;<INDEX>
ide int13fakeio|int13fakeio;false|true;<INDEX>
ide int13fakev86io|int13fakev86io;false|true;<INDEX>
ide enable pio32|enable pio32;false|true;<INDEX>
ide ignore pio32|ignore pio32;false|true;<INDEX>
ide cd-rom spinup time|cd-rom spinup time;0;<INDEX>
ide cd-rom spindown timeout|cd-rom spindown timeout;0;<INDEX>
ide cd-rom insertion delay|cd-rom insertion delay;0;<INDEX>

@Tide` septernary
ide enable|enable;false|true;<INDEX>
ide pnp|pnp;true|false;<INDEX>
ide irq|irq;0|1|2|3|4|5|6;<INDEX>
ide io|io;0|1F0;<INDEX>
ide altio|altio;0|3F6;<INDEX>
ide int13fakeio|int13fakeio;false|true;<INDEX>
ide int13fakev86io|int13fakev86io;false|true;<INDEX>
ide enable pio32|enable pio32;false|true;<INDEX>
ide ignore pio32|ignore pio32;false|true;<INDEX>
ide cd-rom spinup time|cd-rom spinup time;0;<INDEX>
ide cd-rom spindown timeout|cd-rom spindown timeout;0;<INDEX>
ide cd-rom insertion delay|cd-rom insertion delay;0;<INDEX>

@Tide` octernary
ide enable|enable;false|true;<INDEX>
ide pnp|pnp;true|false;<INDEX>
ide irq|irq;0|1|2|3|4|5|6;<INDEX>
ide io|io;0|1F0;<INDEX>
ide altio|altio;0|3F6;<INDEX>
ide int13fakeio|int13fakeio;false|true;<INDEX>
ide int13fakev86io|int13fakev86io;false|true;<INDEX>
ide enable pio32|enable pio32;false|true;<INDEX>
ide ignore pio32|ignore pio32;false|true;<INDEX>
ide cd-rom spinup time|cd-rom spinup time;0;<INDEX>
ide cd-rom spindown timeout|cd-rom spindown timeout;0;<INDEX>
ide cd-rom insertion delay|cd-rom insertion delay;0;<INDEX>
end