[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

If set, and emulating CGA/PCjr/Tandy, automatically provide the second half of the 8x8 ROM font.

This setting is ignored for EGA/VGA emulation. If not set, you will need a utility like GRAFTABL.COM to load the second half of the ROM font for graphics.

NOTE: if you disable the 14 & 16 pixel high font AND the second half when machine=cga, you will disable video bios completely.