[Àû¿ë´ë»ó: 0.74_SVN, 0.74_SVN_new, DOSBox-x]

The physical address the emulator will use on your network.

If you have multiple DOSBoxes running on your network, this has to be changed for each.

AC:DE:48 is an address range reserved for
private use, so modify the last three number blocks.

I.e. AC:DE:48:88:99:AB.