[Àû¿ë´ë»ó: DOSBox-x]

If 0 or greater, apply a delay (in cycles) to IRQ handling in the CPU.

A value of -1 means to use a default value.

There are some old DOS games and demos that have race conditions with IRQs that need a nonzero value here to work properly.