[Àû¿ë´ë»ó: DOSBox-x]

If true, DMA controller emulation models ISA hardware that permits 16-bit DMA to span 128KB.

If false, DMA controller emulation models PCI hardware that limits 16-bit DMA to 64KB boundaries.

If auto, the choice is made according to other factors in hardware emulation

Possible values: true, false, 1, 0, auto.
