[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

If set, keep private DOS segment in upper memory block, usually segment 0xC800 (Mainline DOSBox behavior)

If clear, place private DOS segment at the base of system memory (just below the MCB)