[Àû¿ë´ë»ó: DOSBox-x]

If set, INT 16h function AH=01h will also set/clear the carry flag depending on whether input was available.

There are some old DOS games and demos that rely on this behavior to sense keyboard input, and this behavior has been verified to occur on some old (early 90s) BIOSes.
