[Àû¿ë´ë»ó: DOSBox-x]

If true (default), the DOS kernel will create an alternate interrupt handler for debug interrupts INT 1 and INT 3 that contain ONLY an IRETF instruction.

If false, INT 1 and INT 3 will use the same default interrupt handler in the DOS kernel, which contains a callback instruction followed by IRETF.

Some DOS games/demos assume they are being
debugged if the debug interrupts point to anything other than an IRETF instruction.

Set this option to false if you need notification that INT 1/INT 3 was not handled.
