[Àû¿ë´ë»ó: DOSBox-x]

Start the DOS virtual machine with the DMA channel already unmasked at the controller.

Use this for DOS applications that expect to operate the GUS but forget to unmask the DMA channel.
