[Àû¿ë´ë»ó: DOSBox-x]

VGA status port 3BA/3DAh only defines bits 0 and 3.
This setting allows you to assign a bit pattern to the undefined bits.

The purpose of this hack is to deal with demos that read and handle port 3DAh in ways that might crash if all are zero.

By default, this value is zero.
