[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

DMA channel for floppy controller.
Set to -1 for default.

WARNING: Setting the DMA channel to non-standard values will not work unless the guest OS is using the ISA PnP BIOS to detect the IDE controller.

Standard DMA channel is 2.