[Àû¿ë´ë»ó: DOSBox-x]

Allow TSR and application (anything other than the DOS kernel) to request control of the HMA.

They will not be able to request control however if the DOS kernel is configured to occupy the HMA (DOS=HIGH)
