[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

If set, 32-bit I/O reads and writes are handled directly (much like PCI IDE implementations)

If clear, 32-bit I/O will be handled as if two 16-bit I/O (much like ISA IDE implementations)