[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

If set, allow increment & decrement modes as specified in the 8237 datasheet.

If clear, always increment the address (as if to emulate clone 8237 implementations that skipped the inc/dec bit).