[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

VGA debugging switch. If set, an inverse green dotted line will be drawn on the exact scanline that the CRTC status port (0x3DA) was read.

This can be used to help diagnose whether the DOS game is propertly waiting for vertical retrace.