[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

VGA debugging switch. If set, an inverse line will be drawn on the exact scanline that the CRTC display offset registers were written.

This can be used to help diagnose whether or not the DOS game is page flipping properly according to vertical retrace if the display on-screen is flickering.