[Àû¿ë´ë»ó: DOSBox-x]

IF nonzero, VESA modes with vertical resolution higher than the specified pixel count will not be listed.

This is another way the modelist can be capped for DOS applications that have trouble with long modelists.
