[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

If set, allow low resolution VESA modes (320x200x16/24/32bpp and so on). You could set this to false to simulate SVGA hardware with a BIOS that does not support the lowres modes for testing purposes.