[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

If set, truecolor (16M color) VESA BIOS modes in the 0x100-0x11F range are 32bpp. If clear, they are 24bpp.

Some DOS games and demos assume one bit depth or the other and do not enumerate VESA BIOS modes, which is why this option exists.