[Àû¿ë´ë»ó: DOSBox-x]

Controls which table or equation is used for the Gravis Ultrasound panning emulation.

accurate emulation attempts to better reflect how the actual hardware handles panning,

while the old emulation uses a simpler idealistic mapping.

Possible values: old, accurate, default.