[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

Allow guest OS to connect from 32-bit protected mode.

If you want power management in Windows 95/98/ME (beyond using the APM to shutdown the computer) you MUST enable this option.

Windows 95/98/ME does not support the 16-bit real and protected mode APM BIOS entry points.