[Àû¿ë´ë»ó: DOSBox-x]

If set, automatically enable GUS DMA transfer bit
in specific cases when the DMA control register
is being polled.

THIS IS A HACK. Some games and demoscene
productions need this hack to avoid hanging while
uploading sample data to the Gravis Ultrasound
due to bugs in their implementation.