[Àû¿ë´ë»ó: DOSBox-x]

This setting affects the VGA Line Compare register.

Set to false (default value) to emulate most VGA behavior.

Set to true for the value to latch once at the start of the frame.
