[Àû¿ë´ë»ó: DOSBox-x]

If set and expanded memory is set to emulate emm386, start the DOS machine with EMM386.EXE active(running the 16-bit DOS environment from within Virtual 8086 mode).

If you will be running anything that involves a DOS extender you will also need to enable the VCPI interface as well.
