[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

If set, or mainline compatible bios mapping, a legacy 8x8 CGA font (first 128 characters) is stored at 0xF000:0xFA6E. DOS programs that do not use INT 10h to locate fonts might require that font to be located there.