[Àû¿ë´ë»ó: 0.74_SVN_new, DOSBox-x]

If set, and space is available, allow conventional memory to extend past 640KB.

For example, if machine=cga, conventional memory can extend out to 0xB800 and provide up to 736KB of RAM.

This allows you to emulate PC/XT style memory extensions.