[Àû¿ë´ë»ó: DOSBox-x]

Minimum segment value to begin memory allocation from, in hexadecimal. Set to 0 for default.

You can increase available DOS memory by reducing this value down to as low as 0x51, however setting it to low can cause some DOS programs to crash or run erratically, and some DOS games and demos to cause intermittent static noises when using Sound Blaster output.

DOS programs compressed with Microsoft EXEPACK will not run if the minimum MCB segment is below 64KB.
